Since version 3, it has been possible to remote upload and download settings to the transmitter.
To do this, it is necessary that the transmitter has a permanent connection to the GPRS server.
Required minimum version of GPRS server - 4.0.70. In the GPRS server, you must enter the password in the appropriate field - 8 characters.
In NV PRO, on the NV Online PRO Settings tab, click the GPRS server button and enter the IP address and port of the GPRS server and the password that was entered in the GPRS server.
By clicking on the Sessions button, you can check the connection with the GPRS server and see a list of objects that are currently connected to the server.
Enter the account number of the transmitter whose settings you plan to upload or download.
To check if the name and version of the transmitter match the selected template in the program, click the Device name button.
To upload or download the settings, press the corresponding button.
There are situations when the transmitter is in the list of accounts that are in communication with the GPRS server, but communication with it can not be established.
This can be for several reasons.
The GPRS test time is set to 5 minutes or more. In this case, the transmitter is not in constant connection with the server, it is necessary to set the test time less than 5 minutes.
The transmitter can be busy re-registering in the GSM network if were made several failed attempts to send reports.
The transmitter can be busy sending a periodic test from another SIM card, if such a test is specified in the settings.
After finishing the recording of the settings, do not try to read them immediately, since the transmitter will be unavailable for 2-3 minutes due to reboot and re-registration in the network.
Button Version update.
For the transmitter to update its software version to the most current one, just click the Update version button.
In the Number field, enter the phone number to which the operation notification will be sent.
If you want to update the version to an unofficial one, enter the name of the firmware file in the File field.
Devices for which the NV Online PRO function is available:
8704v06.02.34
8704v05.02.34
226v04.01.54
226v05.01.54
227v04.01.35
228v04.01.35
229v04.01.35
241v04.01.35
290v04.01.35
292v13.01.35
2227v02.01.12
2228v02.01.12
8321v02.01.35
8320v02.01.35
2050v15.01.16
2020v15.01.16
2020v16.01.16